Monday I got a spot we knew how low the tank could go and clamped it. 2 Steps Taken to Reach Objective: Objective (s): Work in lab on year long project and start getting a design for ornament. List issues / Complications: 1 3 4 We sat the body on top on the rear end to see how it would look. I had no complications today. I first started by seeing how low we could get the tank Thought of ideas for body modifications. Tuesday The design was final and we needed to find a material we could use. 2 Steps Taken to Reach Objective: Objective (s): Brainstorm ideas about body modifications for formula car. List issues / Complications: 1 3 4 We got together as a team and discussed what we could use and what would look the best. There were no complications today. I held up paper designs and cardboard designs to the body and decided which one we all liked better.
We Wednesday I cut out the slots so the body and the nose cone was not in the way of the steering. 2 Steps Taken to Reach Objective: Objective (s): Work in lab on year long project. List issues / Complications: 1 3 4 All the cuts fit and I bolted the nose cone to the front to see when it supported itself if steering would work. No complications today. First I took measurements to see how much we needed to cut out of the nose cone. Thursday We marked our lines on the sheet metal and used the electric shears to cut it out. 2 Steps Taken to Reach Objective: Objective (s): Work on formula body mods List issues / Complications: 1 3 4 I got L-brackets so we could mount the sheet metal to the plexi-glass piece we cut. I had no complications today. I took all of the measurements we needed to take so we could cut out the sheet metal for the body . Friday I got all the wires attached and hooked up correctly 2 Steps Taken to Reach Objective: Objective (s): Work in lab on year long project work on ornament design List issues / Complications: 1 3 4 I checked for wire flaws and found none. We could not get a locknut off of the di-ode bolt. I worked on re-wiring the engine and the tach light.